;-------------------------------------------------------------------------------
;
; BYPUSB.INF  --	Windows USB Printer Device Driver
;
; Copyright(C) 2001-2017 Shandong New Beiyang Information Technology Co., Ltd. 
;
;-------------------------------------------------------------------------------

[Version]
Signature = "$CHICAGO$"
Class     = USB
ClassGUID = {36FC9E60-C465-11CF-8056-444553540000}
provider  = SNBC
CatalogFile =BYPUSB.cat
DriverVer = 08/17/2017,3.2.1.0
LayoutFile= layout.inf

[Manufacturer]
%Device.MfgSNBC%=ModelsSNBC,NTx86,NTamd64

[ModelsSNBC]
; POS/KIOSK Printers
%USB\SNBC.POSPrinterDesc%=Device.Printer, USB\VID_154F&PID_154F
%USB\SNBC.POSPrinterDesc%=Device.Printer, USB\VID_04ce&PID_04ce
%USB\SNBC.POSPrinterDesc%=Device.Printer, USB\VID_154F&PID_1001

;label printer pid_1000
%USB\SNBC.LabelPrinterDesc%=Device.Printer, USB\VID_154F&PID_1000

;General printer
%USB\SNBC.PrinterDesc%=Device.Printer, USB\VID_154F&PID_1002

[ModelsSNBC.NTx86]
; POS/KIOSK Printers
%USB\SNBC.POSPrinterDesc%=Device.Printer, USB\VID_154F&PID_154F
%USB\SNBC.POSPrinterDesc%=Device.Printer, USB\VID_04ce&PID_04ce
%USB\SNBC.POSPrinterDesc%=Device.Printer, USB\VID_154F&PID_1001

;label printer pid_1000
%USB\SNBC.LabelPrinterDesc%=Device.Printer, USB\VID_154F&PID_1000

;General printer
%USB\SNBC.PrinterDesc%=Device.Printer, USB\VID_154F&PID_1002

[ModelsSNBC.NTamd64]
; POS/KIOSK Printers
%USB\SNBC.POSPrinterDesc%=Device.Printer, USB\VID_154F&PID_154F
%USB\SNBC.POSPrinterDesc%=Device.Printer, USB\VID_04ce&PID_04ce
%USB\SNBC.POSPrinterDesc%=Device.Printer, USB\VID_154F&PID_1001

;label printer pid_1000
%USB\SNBC.LabelPrinterDesc%=Device.Printer, USB\VID_154F&PID_1000

;General printer
%USB\SNBC.PrinterDesc%=Device.Printer, USB\VID_154F&PID_1002

[PreCopySection]
HKR,,NoSetupUI,,1

[DestinationDirs]
BYPUSB.Files.Ext = 10,System32\Drivers

[Device.Printer]
CopyFiles=BYPUSB.Files.Ext
AddReg=BYPUSB.AddReg

[Device.Printer.NTx86]
CopyFiles=BYPUSB.Files.Ext
AddReg=BYPUSB.AddReg

[Device.Printer.NTx86.Services]
Addservice = BYPUSB, 0x00000002, BYPUSB.AddService

[Device.Printer.NTamd64]
CopyFiles=BYPUSB.Files.Ext 
AddReg=BYPUSB.AddReg

[Device.Printer.NTamd64.Services]
Addservice = BYPUSB, 0x00000002, BYPUSB.AddService

[BYPUSB.AddService]
DisplayName    = %BYPUSB.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ;SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\BYPUSB.sys
LoadOrderGroup = Base

[BYPUSB.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,BYPUSB.sys
;HKLM,"System\Currentcontrolset\Services\BYPUSB\Parameters","MaximumTransferSize",0x10001,4096
;HKLM,"System\Currentcontrolset\Services\BYPUSB\Parameters","DebugLevel",0x10001,2

HKLM,"SOFTWARE\BEIYANG\PRINTERPORT","D1",0x10001,
HKLM,"SOFTWARE\BEIYANG\PRINTERPORT","D2",0x10001,
HKLM,"SOFTWARE\BEIYANG\PRINTERPORT","D3",0x10001,
HKLM,"SOFTWARE\BEIYANG\PRINTERPORT","D4",0x10001,
HKLM,"SOFTWARE\BEIYANG\PRINTERPORT","D5",0x10001,
HKLM,"SOFTWARE\BEIYANG\PRINTERPORT","D6",0x10001,
HKLM,"SOFTWARE\BEIYANG\PRINTERPORT","D7",0x10001,
HKLM,"SOFTWARE\BEIYANG\PRINTERPORT","D8",0x10001,


[BYPUSB.Files.Ext]
BYPUSB.sys

[SourceDisksFiles]
BYPUSB.sys=99

[SourceDisksNames]
99=%Disk%,,


;-------------------------------------------------------------------------------
;
; Strings section - Always put strings down here so they can be easily localized 
; to other languages
;
;-------------------------------------------------------------------------------

[Strings]
Provider="SNBC"
Device.MfgSNBC="Shandong New Beiyang Information Technology Co., Ltd"
USB\SNBC.POSPrinterDesc="USB Device Driver for POS/KIOSK Printers"
USB\SNBC.LabelPrinterDesc="USB Device Driver for Label Printers"
USB\SNBC.PrinterDesc="SNBC Printer USB Device Driver"
BYPUSB.SvcDesc="SNBC Printer USB Device Driver"
Disk="SNBC Printer Driver"
